**SPROCKET CALCULATIONS**

No. of teeth=9

Pitch=12.5mm

Outer Diameter=pitch(0.6+cot(180/n), n=no. of teeth

=41.84 mm

Pitch Diameter=pitch/sin(180/n)

=36.54 mm